$Id: TODO,v 1.13 2003/09/15 17:31:46 telka Exp $

* Write documentation.
* Support for displaying the result of a boundary scan formatted according to the CPU definitions (e.g. MA[0-26] = 0x00001c00).
* Remove direct relation between JTAG instruction and data register (e.g. ARM7TDMI).
* SVF player.
